# 1.1 Test results

The result table mentions only the worst cases. For the details see complete tables in the measurements and curves.

# Sample n°CRE2-2025-TP002-02

## Configuration ER\_In front of harness RBW 9kHz

Paramètres de test :

• Project: CRE2-2025-TP002 RESAC

• Operator: Operator:

• Test Configuration: Test Configuration:

• Operating mode: Operating mode:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Section** | **Frequency (MHz)** | **SR** | **Polarization** | **Correction (dB)** | **Mesure (dBµV/m)** | **Limite (dBµV/m)** | **Marge (dB)** | **Verdict** |
| Peak | 1.25875 | 1.0 | Vertical | 9.92 | -30.75 | - | N/A | - |
| Peak | 27.269 | 2.0 | Vertical | 10.29 | -35.85 | - | N/A | - |
| Peak | 1.25650 | 1.0 | Vertical | 9.92 | -19.61 | - | N/A | - |
| Peak | 27.260 | 2.0 | Vertical | 10.29 | -28.95 | - | N/A | - |
| Peak | 1.25875 | 1.0 | Vertical | 9.92 | -17.75 | - | N/A | - |
| Peak | 27.269 | 2.0 | Vertical | 10.29 | -22.85 | - | N/A | - |
| CISPR.AVG | 1.25425 | 1.0 | Vertical | 9.92 | -25.65 | 44.0 | 69.65 | OK |
| CISPR.AVG | 27.260 | 2.0 | Vertical | 10.29 | -23.43 | 28.0 | 51.43 | OK |

## Configuration ER\_In front of harness RBW 9kHz\_GNSS

Paramètres de test :

• Project: CRE2-2025-TP002 RESAC

• Operator: Operator:

• Test Configuration: Test Configuration:

• Operating mode: Operating mode:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Section** | **Frequency (MHz)** | **SR** | **Polarization** | **Correction (dB)** | **Mesure (dBµV/m)** | **Limite (dBµV/m)** | **Marge (dB)** | **Verdict** |

Aucune donnée disponible pour cette configuration.

## Configuration ER\_In front of DUT RBW 9kHz\_GNSS

Paramètres de test :

• Project: CRE2-2025-TP002 RESAC

• Operator: Operator:

• Test Configuration: Test Configuration:

• Operating mode: Operating mode:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Section** | **Frequency (MHz)** | **SR** | **Polarization** | **Correction (dB)** | **Mesure (dBµV/m)** | **Limite (dBµV/m)** | **Marge (dB)** | **Verdict** |

Aucune donnée disponible pour cette configuration.

## Configuration ER\_In front of harness RBW 120kHz With PA

Paramètres de test :

• Project: CRE2-2025-TP002 RESAC

• Operator: Operator:

• Test Configuration: Test Configuration:

• Operating mode: Operating mode:

|  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- |
| **Section** | **Frequency (MHz)** | **SR** | **Polarization** | **Correction (dB)** | **Mesure (dBµV/m)** | **Limite (dBµV/m)** | **Marge (dB)** | **Verdict** |

Aucune donnée disponible pour cette configuration.